1. Wireless Internet is available and ubiquitous.
   1. All Beta Nodes.
2. Wired Internet is available and ubiquitous.
   1. One Gamma Node should pick Ethernet from available wired network. The other Beta Nodes must communicate their data to the Gamma Gateway via Zigbee or some other RF mesh network protocol.
3. Wired Network is available but not Internet.
4. Wireless Network is available but not Internet.
5. Not Network is available.